60W 30W 0

EQ.

15S

15N

Xie and Arkin gridpoints used for FQI update